

NTRIPServer Configuration

* NTRIP Server


Step1. click ‘Option’




Step2. Configuration by Mark,then click ‘Setup’




Step3. Configuration by Mark,click ‘save’




Step4.click Start



Then, You will see the data sent successful



* NTRIP Client



The NTRIP delay is marked in the figure.